{
  "schema_version": "1.4.0",
  "id": "GHSA-v9r3-74m9-xhvh",
  "modified": "2022-05-14T03:28:42Z",
  "published": "2022-05-14T03:28:42Z",
  "aliases": [
    "CVE-2016-10450"
  ],
  "details": "In Android before 2018-04-05 or earlier security patch level on Qualcomm Small Cell SoC, Snapdragon Mobile, and Snapdragon Wear FSM9055, MDM9206, MDM9607, MDM9635M, MDM9640, MDM9650, MSM8909W, SD 210/SD 212/SD 205, SD 400, SD 410/12, SD 425, SD 430, SD 450, SD 615/16/SD 415, SD 617, SD 625, SD 650/52, SD 800, SD 808, SD 810, SD 820, SD 835, and SDX20, potential stack-based buffer overflow exist in thermal service leading to root compromise.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2016-10450"
    },
    {
      "type": "WEB",
      "url": "https://source.android.com/security/bulletin/2018-04-01"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/103671"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "CRITICAL",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-04-18T14:29:00Z"
  }
}