{
  "schema_version": "1.4.0",
  "id": "GHSA-vqjf-hc9h-q7qc",
  "modified": "2022-05-14T02:15:26Z",
  "published": "2022-05-14T02:15:26Z",
  "aliases": [
    "CVE-2010-2817"
  ],
  "details": "Unspecified vulnerability in the IKE implementation on Cisco Adaptive Security Appliances (ASA) 5500 series devices with software 7.0 before 7.0(8.11), 7.1 and 7.2 before 7.2(5), 8.0 before 8.0(5.15), 8.1 before 8.1(2.44), 8.2 before 8.2(2.10), and 8.3 before 8.3(1.1) and Cisco PIX Security Appliances 500 series devices allows remote attackers to cause a denial of service (device reload) via a crafted IKE message, aka Bug ID CSCte46507.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2010-2817"
    },
    {
      "type": "WEB",
      "url": "http://secunia.com/advisories/40842"
    },
    {
      "type": "WEB",
      "url": "http://www.cisco.com/en/US/products/products_security_advisory09186a0080b3f12f.shtml"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/42190"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2010-08-09T11:58:00Z"
  }
}