# master 0 

canonical_ip: 10.153.7.109
interface_IPs:
  intapi:
    bmc_id: NIC2
    bmc_name: External Ethernet Interface
    interface: ens9f1
    ipv4: 10.153.6.10.109
    macaddress: E4:3D:1A:62:FB:A9
    vlan: '1181'
  ocp:
    bmc_id: NIC3
    bmc_name: External Ethernet Interface
    interface: ens9f2
    ipv4: 10.153.11.109
    macaddress: E4:3D:1A:62:FB:AA
  outside:
    bmc_id: NIC2
    bmc_name: External Ethernet Interface
    interface: ens9f1
    macaddress: E4:3D:1A:62:FB:A9
    vlan: '1183'
  pxe:
    bmc_id: NIC4
    bmc_name: External Ethernet Interface
    interface: ens9f3
    ipv4: 10.153.15.109
    macaddress: E4:3D:1A:62:FB:AB
  tenant:
    bmc_id: NIC2
    bmc_name: External Ethernet Interface
    interface: ens9f1
    ipv4: 10.153.9.109
    macaddress: E4:3D:1A:62:FB:A9
    vlan: '1180'
ipmi:
  ip_address: 192.168.208.149
