{
  "schema_version": "1.4.0",
  "id": "GHSA-2968-fmvc-r6gw",
  "modified": "2024-04-04T03:27:36Z",
  "published": "2023-04-14T03:30:28Z",
  "aliases": [
    "CVE-2023-1285"
  ],
  "details": "Signal Handler Race Condition vulnerability in Mitsubishi Electric India GC-ENET-COM whose first 2 digits of 11-digit serial number of unit are \"16\" allows a remote unauthenticated attacker to cause a denial-of-service (DoS) condition in Ethernet communication by sending a large number of specially crafted packets to any UDP port when GC-ENET-COM is configured as a Modbus TCP Server. The communication resumes only when the power of the main unit is turned off and on or when the GC-ENET-COM is hot-swapped from the main unit.\n",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:N/AC:H/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2023-1285"
    },
    {
      "type": "WEB",
      "url": "https://mitsubishielectric.in/fa/cnc-pdf/DoS_in_Ethernet_Communication_Extension_Unit_GC_ENET_COM_of_GOC35_Series.pdf"
    },
    {
      "type": "WEB",
      "url": "https://www.cisa.gov/news-events/ics-advisories/icsa-23-103-15"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-362",
      "CWE-364"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2023-04-14T03:15:00Z"
  }
}