{
  "schema_version": "1.4.0",
  "id": "GHSA-h5hc-qpqf-p7r8",
  "modified": "2024-04-04T03:31:12Z",
  "published": "2023-04-18T00:32:00Z",
  "aliases": [
    "CVE-2023-28959"
  ],
  "details": "An Improper Check or Handling of Exceptional Conditions vulnerability in packet processing of Juniper Networks Junos OS on QFX10002 allows an unauthenticated, adjacent attacker on the local broadcast domain sending a malformed packet to the device, causing all PFEs other than the inbound PFE to wedge and to eventually restart, resulting in a Denial of Service (DoS) condition. Continued receipt and processing of this packet will create a sustained Denial of Service (DoS) condition. This issue can only be triggered by sending a specific malformed packet to the device. Transit traffic does not trigger this issue. An indication of this issue occurring can be seen through the following log messages: fpc0 expr_hostbound_packet_handler: Receive pe 73? fpc0 Cmerror Op Set: PE Chip: PE0[0]: PGQ:misc_intr: 0x00000020: Enqueue of a packet with out-of-range VOQ in 192K-VOQ mode (URI: /fpc/0/pfe/0/cm/0/PE_Chip/0/PECHIP_CMERROR_PGQ_MISC_INT_EVENTS_ENQ_192K_VIOL) The logs list below can also be observed when this issue occurs fpc0 Error: /fpc/0/pfe/0/cm/0/PE_Chip/0/PECHIP_CMERROR_PGQ_MISC_INT_EVENTS_ENQ_192K_VIOL (0x210107), scope: pfe, category: functional, severity: major, module: PE Chip, type: Description for PECHIP_CMERROR_PGQ_MISC_INT_EVENTS_ENQ_192K_VIOL fpc0 Performing action cmalarm for error /fpc/0/pfe/0/cm/0/PE_Chip/0/PECHIP_CMERROR_PGQ_MISC_INT_EVENTS_ENQ_192K_VIOL (0x210107) in module: PE Chip with scope: pfe category: functional level: major fpc0 Error: /fpc/0/pfe/0/cm/0/PE_Chip/0/PECHIP_CMERROR_CM_INT_REG_DCHK_PIPE (0x21011a), scope: pfe, category: functional, severity: fatal, module: PE Chip, type: Description for PECHIP_CMERROR_CM_INT_REG_DCHK_PIPE fpc0 Performing action cmalarm for error /fpc/0/pfe/0/cm/0/PE_Chip/0/PECHIP_CMERROR_CM_INT_REG_DCHK_PIPE (0x21011a) in module: PE Chip with scope: pfe category: functional level: fatal fpc0 Performing action disable-pfe for error /fpc/0/pfe/0/cm/0/PE_Chip/0/PECHIP_CMERROR_CM_INT_REG_DCHK_PIPE (0x21011a) in module: PE Chip with scope: pfe category: functional level: fatal This issue affects Juniper Networks Junos OS on QFX10002: All versions prior to 19.1R3-S10; 19.4 versions prior to 19.4R3-S11; 20.2 versions prior to 20.2R3-S7; 20.4 versions prior to 20.4R3-S6; 21.1 versions prior to 21.1R3-S4; 21.2 versions prior to 21.2R3-S4; 21.3 versions prior to 21.3R3-S3; 21.4 versions prior to 21.4R3-S2; 22.1 versions prior to 22.1R3-S1; 22.2 versions prior to 22.2R2-S1, 22.2R3; 22.3 versions prior to 22.3R1-S2, 22.3R2.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:A/AC:L/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2023-28959"
    },
    {
      "type": "WEB",
      "url": "https://supportportal.juniper.net/JSA70584"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-703"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2023-04-17T22:15:08Z"
  }
}