{
  "schema_version": "1.4.0",
  "id": "GHSA-j4pp-rp58-2qhj",
  "modified": "2024-04-04T03:36:30Z",
  "published": "2023-04-20T00:30:43Z",
  "aliases": [
    "CVE-2023-23451"
  ],
  "details": "The Flexi Classic and Flexi Soft Gateways SICK UE410-EN3 FLEXI ETHERNET GATEW., SICK UE410-EN1 FLEXI ETHERNET GATEW., SICK UE410-EN3S04 FLEXI ETHERNET GATEW., SICK UE410-EN4 FLEXI ETHERNET GATEW., SICK FX0-GENT00000 FLEXISOFT EIP GATEW., SICK FX0-GMOD00000 FLEXISOFT MOD GATEW., SICK FX0-GPNT00000 FLEXISOFT PNET GATEW., SICK FX0-GENT00030 FLEXISOFT EIP GATEW.V2, SICK FX0-GPNT00030 FLEXISOFT PNET GATEW.V2 and SICK FX0-GMOD00010 FLEXISOFT MOD GW. have Telnet enabled by factory default. No password is set in the default configuration. Gateways with a serial number >2311xxxx have the Telnet interface disabled by factory default.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:N/AC:L/PR:N/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2023-23451"
    },
    {
      "type": "WEB",
      "url": "https://sick.com/psirt"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-306",
      "CWE-477"
    ],
    "severity": "CRITICAL",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2023-04-19T23:15:06Z"
  }
}