 with + or (if there are 2 operands) a digit.
An OFFSET operand means -j OFFSET.  LABEL is the pseudo-address
at first byte printed, incremented when dump is progressing.
For OFFSET and LABEL, a 0x or 0X prefix indicates hexadecimal;
suffixes may be . for octal and b for multiply by 512.
