{
  "schema_version": "1.4.0",
  "id": "GHSA-2hx9-gcpq-rv3h",
  "modified": "2022-05-17T01:53:20Z",
  "published": "2022-05-17T01:53:20Z",
  "aliases": [
    "CVE-2011-3491"
  ],
  "details": "Heap-based buffer overflow in Progea Movicon / PowerHMI 11.2.1085 and earlier allows remote attackers to cause a denial of service (crash) and possibly execute arbitrary code via a negative Content-Length field.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2011-3491"
    },
    {
      "type": "WEB",
      "url": "https://exchange.xforce.ibmcloud.com/vulnerabilities/69787"
    },
    {
      "type": "WEB",
      "url": "http://aluigi.altervista.org/adv/movicon_1-adv.txt"
    },
    {
      "type": "WEB",
      "url": "http://osvdb.org/75494"
    },
    {
      "type": "WEB",
      "url": "http://www.us-cert.gov/control_systems/pdf/ICS-ALERT-11-256-01.pdf"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2011-09-16T14:28:00Z"
  }
}