[
    {
        "BriefDescription": "Counts the number of core requests (demand and L1 prefetchers) rejected by the L2 queue (L2Q) due to a full condition.",
        "Counter": "0,1,2,3",
        "EventCode": "0x31",
        "EventName": "CORE_REJECT_L2Q.ANY",
        "PublicDescription": "Counts the number of (demand and L1 prefetchers) core requests rejected by the L2 queue (L2Q) due to a full or nearly full condition, which likely indicates back pressure from L2Q.  It also counts requests that would have gone directly to the External Queue (XQ), but are rejected due to a full or nearly full condition, indicating back pressure from the IDI link.  The L2Q may also reject transactions  from a core to ensure fairness between cores, or to delay a cores dirty eviction when the address conflicts incoming external snoops.  (Note that L2 prefetcher requests that are dropped are not counted by this event).  Counts on a per core basis.",
        "SampleAfterValue": "200003"
    },
    {
        "BriefDescription": "Counts the number of L1D cacheline (dirty) evictions caused by load misses, stores, and prefetches.",
        "Counter": "0,1,2,3",
        "EventCode": "0x51",
        "EventName": "DL1.DIRTY_EVICTION",
        "PublicDescription": "Counts the number of L1D cacheline (dirty) evictions caused by load misses, stores, and prefetches.  Does not count evictions or dirty writebacks caused by snoops.  Does not count a replacement unless a (dirty) line was written back.",
        "SampleAfterValue": "200003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts the number of demand and prefetch transactions that the External Queue (XQ) rejects due to a full or near full condition.",
        "Counter": "0,1,2,3",
        "EventCode": "0x30",
        "EventName": "L2_REJECT_XQ.ANY",
        "PublicDescription": "Counts the number of demand and prefetch transactions that the External Queue (XQ) rejects due to a full or near full condition which likely indicates back pressure from the IDI link.  The XQ may reject transactions from the L2Q (non-cacheable requests), BBL (L2 misses) and WOB (L2 write-back victims).",
        "SampleAfterValue": "200003"
    },
    {
        "BriefDescription": "Counts the total number of L2 Cache accesses. Counts on a per core basis.",
        "Counter": "0,1,2,3",
        "EventCode": "0x24",
        "EventName": "L2_REQUEST.ALL",
        "PublicDescription": "Counts the total number of L2 Cache Accesses, includes hits, misses, rejects  front door requests for CRd/DRd/RFO/ItoM/L2 Prefetches only.  Counts on a per core basis.",
        "SampleAfterValue": "200003"
    },
    {
        "BriefDescription": "Counts the number of L2 Cache accesses that resulted in a hit. Counts on a per core basis.",
        "Counter": "0,1,2,3",
        "EventCode": "0x24",
        "EventName": "L2_REQUEST.HIT",
        "PublicDescription": "Counts the number of L2 Cache accesses that resulted in a hit from a front door request only (does not include rejects or recycles), Counts on a per core basis.",
        "SampleAfterValue": "200003",
        "UMask": "0x2"
    },
    {
        "BriefDescription": "Counts the number of L2 Cache accesses that resulted in a miss. Counts on a per core basis.",
        "Counter": "0,1,2,3",
        "EventCode": "0x24",
        "EventName": "L2_REQUEST.MISS",
        "PublicDescription": "Counts the number of L2 Cache accesses that resulted in a miss from a front door request only (does not include rejects or recycles). Counts on a per core basis.",
        "SampleAfterValue": "200003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts the number of L2 Cache accesses that miss the L2 and get rejected. Counts on a per core basis.",
        "Counter": "0,1,2,3",
        "EventCode": "0x24",
        "EventName": "L2_REQUEST.REJECTS",
        "PublicDescription": "Counts the number of L2 Cache accesses that miss the L2 and get BBL reject  short and long rejects (includes those counted in L2_reject_XQ.any). Counts on a per core basis.",
        "SampleAfterValue": "200003",
        "UMask": "0x4"
    },
    {
        "BriefDescription": "Counts the number of cacheable memory requests that miss in the LLC. Counts on a per core basis.",
        "Counter": "0,1,2,3",
        "EventCode": "0x2e",
        "EventName": "LONGEST_LAT_CACHE.MISS",
        "PublicDescription": "Counts the number of cacheable memory requests that miss in the Last Level Cache (LLC). Requests include demand loads, reads for ownership (RFO), instruction fetches and L1 HW prefetches. If the platform has an L3 cache, the LLC is the L3 cache, otherwise it is the L2 cache. Counts on a per core basis.",
        "SampleAfterValue": "200003",
        "UMask": "0x41"
    },
    {
        "BriefDescription": "Counts the number of cacheable memory requests that access the LLC. Counts on a per core basis.",
        "Counter": "0,1,2,3",
        "EventCode": "0x2e",
        "EventName": "LONGEST_LAT_CACHE.REFERENCE",
        "PublicDescription": "Counts the number of cacheable memory requests that access the Last Level Cache (LLC). Requests include demand loads, reads for ownership (RFO), instruction fetches and L1 HW prefetches. If the platform has an L3 cache, the LLC is the L3 cache, otherwise it is the L2 cache. Counts on a per core basis.",
        "SampleAfterValue": "200003",
        "UMask": "0x4f"
    },
    {
        "BriefDescription": "Counts the number of cycles the core is stalled due to an instruction cache or TLB miss which hit in the L2, LLC, DRAM or MMIO (Non-DRAM).",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "MEM_BOUND_STALLS.IFETCH",
        "PublicDescription": "Counts the number of cycles the core is stalled due to an instruction cache or translation lookaside buffer (TLB) miss which hit in the L2, LLC, DRAM or MMIO (Non-DRAM).",
        "SampleAfterValue": "200003",
        "UMask": "0x38"
    },
    {
        "BriefDescription": "Counts the number of cycles the core is stalled due to an instruction cache or TLB miss which hit in DRAM or MMIO (Non-DRAM).",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "MEM_BOUND_STALLS.IFETCH_DRAM_HIT",
        "PublicDescription": "Counts the number of cycles the core is stalled due to an instruction cache or translation lookaside buffer (TLB) miss which hit in DRAM or MMIO (non-DRAM).",
        "SampleAfterValue": "200003",
        "UMask": "0x20"
    },
    {
        "BriefDescription": "Counts the number of cycles the core is stalled due to an instruction cache or TLB miss which hit in the L2 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "MEM_BOUND_STALLS.IFETCH_L2_HIT",
        "PublicDescription": "Counts the number of cycles the core is stalled due to an instruction cache or Translation Lookaside Buffer (TLB) miss which hit in the L2 cache.",
        "SampleAfterValue": "200003",
        "UMask": "0x8"
    },
    {
        "BriefDescription": "Counts the number of cycles the core is stalled due to an instruction cache or TLB miss which hit in the LLC or other core with HITE/F/M.",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "MEM_BOUND_STALLS.IFETCH_LLC_HIT",
        "PublicDescription": "Counts the number of cycles the core is stalled due to an instruction cache or Translation Lookaside Buffer (TLB) miss which hit in the Last Level Cache (LLC) or other core with HITE/F/M.",
        "SampleAfterValue": "200003",
        "UMask": "0x10"
    },
    {
        "BriefDescription": "Counts the number of cycles the core is stalled due to a demand load miss which hit in the L2, LLC, DRAM or MMIO (Non-DRAM).",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "MEM_BOUND_STALLS.LOAD",
        "SampleAfterValue": "200003",
        "UMask": "0x7"
    },
    {
        "BriefDescription": "Counts the number of cycles the core is stalled due to a demand load miss which hit in DRAM or MMIO (Non-DRAM).",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "MEM_BOUND_STALLS.LOAD_DRAM_HIT",
        "SampleAfterValue": "200003",
        "UMask": "0x4"
    },
    {
        "BriefDescription": "Counts the number of cycles the core is stalled due to a demand load which hit in the L2 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "MEM_BOUND_STALLS.LOAD_L2_HIT",
        "SampleAfterValue": "200003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts the number of cycles the core is stalled due to a demand load which hit in the LLC or other core with HITE/F/M.",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "MEM_BOUND_STALLS.LOAD_LLC_HIT",
        "PublicDescription": "Counts the number of cycles the core is stalled due to a demand load which hit in the Last Level Cache (LLC) or other core with HITE/F/M.",
        "SampleAfterValue": "200003",
        "UMask": "0x2"
    },
    {
        "BriefDescription": "Counts the number of cycles the core is stalled due to a store buffer being full.",
        "Counter": "0,1,2,3",
        "EventCode": "0x34",
        "EventName": "MEM_BOUND_STALLS.STORE_BUFFER_FULL",
        "SampleAfterValue": "200003",
        "UMask": "0x40"
    },
    {
        "BriefDescription": "Counts the number of load uops retired that hit in DRAM.",
        "Counter": "0,1,2,3",
        "Data_LA": "1",
        "EventCode": "0xd1",
        "EventName": "MEM_LOAD_UOPS_RETIRED.DRAM_HIT",
        "PEBS": "1",
        "PublicDescription": "Counts the number of load uops retired that hit in DRAM. Available PDIST counters: 0",
        "SampleAfterValue": "200003",
        "UMask": "0x80"
    },
    {
        "BriefDescription": "Counts the number of load uops retired that hit in the L3 cache, in which a snoop was required and modified data was forwarded from another core or module.",
        "Counter": "0,1,2,3",
        "Data_LA": "1",
        "EventCode": "0xd1",
        "EventName": "MEM_LOAD_UOPS_RETIRED.HITM",
        "PEBS": "1",
        "PublicDescription": "Counts the number of load uops retired that hit in the L3 cache, in which a snoop was required and modified data was forwarded from another core or module. Available PDIST counters: 0",
        "SampleAfterValue": "200003",
        "UMask": "0x20"
    },
    {
        "BriefDescription": "Counts the number of load uops retired that hit in the L1 data cache.",
        "Counter": "0,1,2,3",
        "Data_LA": "1",
        "EventCode": "0xd1",
        "EventName": "MEM_LOAD_UOPS_RETIRED.L1_HIT",
        "PEBS": "1",
        "PublicDescription": "Counts the number of load uops retired that hit in the L1 data cache. Available PDIST counters: 0",
        "SampleAfterValue": "200003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts the number of load uops retired that miss in the L1 data cache.",
        "Counter": "0,1,2,3",
        "Data_LA": "1",
        "EventCode": "0xd1",
        "EventName": "MEM_LOAD_UOPS_RETIRED.L1_MISS",
        "PEBS": "1",
        "PublicDescription": "Counts the number of load uops retired that miss in the L1 data cache. Available PDIST counters: 0",
        "SampleAfterValue": "200003",
        "UMask": "0x8"
    },
    {
        "BriefDescription": "Counts the number of load uops retired that hit in the L2 cache.",
        "Counter": "0,1,2,3",
        "Data_LA": "1",
        "EventCode": "0xd1",
        "EventName": "MEM_LOAD_UOPS_RETIRED.L2_HIT",
        "PEBS": "1",
        "PublicDescription": "Counts the number of load uops retired that hit in the L2 cache. Available PDIST counters: 0",
        "SampleAfterValue": "200003",
        "UMask": "0x2"
    },
    {
        "BriefDescription": "Counts the number of load uops retired that miss in the L2 cache.",
        "Counter": "0,1,2,3",
        "Data_LA": "1",
        "EventCode": "0xd1",
        "EventName": "MEM_LOAD_UOPS_RETIRED.L2_MISS",
        "PEBS": "1",
        "PublicDescription": "Counts the number of load uops retired that miss in the L2 cache. Available PDIST counters: 0",
        "SampleAfterValue": "200003",
        "UMask": "0x10"
    },
    {
        "BriefDescription": "Counts the number of load uops retired that hit in the L3 cache.",
        "Counter": "0,1,2,3",
        "Data_LA": "1",
        "EventCode": "0xd1",
        "EventName": "MEM_LOAD_UOPS_RETIRED.L3_HIT",
        "PEBS": "1",
        "PublicDescription": "Counts the number of load uops retired that hit in the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "200003",
        "UMask": "0x4"
    },
    {
        "BriefDescription": "Counts the number of memory uops retired.",
        "Counter": "0,1,2,3",
        "Data_LA": "1",
        "EventCode": "0xd0",
        "EventName": "MEM_UOPS_RETIRED.ALL",
        "PEBS": "1",
        "PublicDescription": "Counts the number of memory uops retired.  A single uop that performs both a load AND a store will be counted as 1, not 2 (e.g. ADD [mem], CONST) Available PDIST counters: 0",
        "SampleAfterValue": "200003",
        "UMask": "0x83"
    },
    {
        "BriefDescription": "Counts the number of load uops retired.",
        "Counter": "0,1,2,3",
        "Data_LA": "1",
        "EventCode": "0xd0",
        "EventName": "MEM_UOPS_RETIRED.ALL_LOADS",
        "PEBS": "1",
        "PublicDescription": "Counts the total number of load uops retired. Available PDIST counters: 0",
        "SampleAfterValue": "200003",
        "UMask": "0x81"
    },
    {
        "BriefDescription": "Counts the number of store uops retired.",
        "Counter": "0,1,2,3",
        "Data_LA": "1",
        "EventCode": "0xd0",
        "EventName": "MEM_UOPS_RETIRED.ALL_STORES",
        "PEBS": "1",
        "PublicDescription": "Counts the total number of store uops retired. Available PDIST counters: 0",
        "SampleAfterValue": "200003",
        "UMask": "0x82"
    },
    {
        "BriefDescription": "Counts the number of load uops retired that performed one or more locks.",
        "Counter": "0,1,2,3",
        "Data_LA": "1",
        "EventCode": "0xd0",
        "EventName": "MEM_UOPS_RETIRED.LOCK_LOADS",
        "PEBS": "1",
        "PublicDescription": "Counts the number of load uops retired that performed one or more locks. Available PDIST counters: 0",
        "SampleAfterValue": "200003",
        "UMask": "0x21"
    },
    {
        "BriefDescription": "Counts the number of memory uops retired that were splits.",
        "Counter": "0,1,2,3",
        "Data_LA": "1",
        "EventCode": "0xd0",
        "EventName": "MEM_UOPS_RETIRED.SPLIT",
        "PEBS": "1",
        "PublicDescription": "Counts the number of memory uops retired that were splits. Available PDIST counters: 0",
        "SampleAfterValue": "200003",
        "UMask": "0x43"
    },
    {
        "BriefDescription": "Counts the number of retired split load uops.",
        "Counter": "0,1,2,3",
        "Data_LA": "1",
        "EventCode": "0xd0",
        "EventName": "MEM_UOPS_RETIRED.SPLIT_LOADS",
        "PEBS": "1",
        "PublicDescription": "Counts the number of retired split load uops. Available PDIST counters: 0",
        "SampleAfterValue": "200003",
        "UMask": "0x41"
    },
    {
        "BriefDescription": "Counts the number of retired split store uops.",
        "Counter": "0,1,2,3",
        "Data_LA": "1",
        "EventCode": "0xd0",
        "EventName": "MEM_UOPS_RETIRED.SPLIT_STORES",
        "PEBS": "1",
        "PublicDescription": "Counts the number of retired split store uops. Available PDIST counters: 0",
        "SampleAfterValue": "200003",
        "UMask": "0x42"
    },
    {
        "BriefDescription": "Counts all code reads that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.ALL_CODE_RD.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1F803C0044",
        "PublicDescription": "Counts all code reads that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts all code reads that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.ALL_CODE_RD.L3_HIT.SNOOP_HITM",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10003C0044",
        "PublicDescription": "Counts all code reads that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts all code reads that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.ALL_CODE_RD.L3_HIT.SNOOP_HIT_NO_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x4003C0044",
        "PublicDescription": "Counts all code reads that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts all code reads that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.ALL_CODE_RD.L3_HIT.SNOOP_HIT_WITH_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x8003C0044",
        "PublicDescription": "Counts all code reads that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts all code reads that were supplied by the L3 cache where a snoop was sent but the snoop missed.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.ALL_CODE_RD.L3_HIT.SNOOP_MISS",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x2003C0044",
        "PublicDescription": "Counts all code reads that were supplied by the L3 cache where a snoop was sent but the snoop missed. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts all code reads that were supplied by the L3 cache where no snoop was needed to satisfy the request.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.ALL_CODE_RD.L3_HIT.SNOOP_NOT_NEEDED",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1003C0044",
        "PublicDescription": "Counts all code reads that were supplied by the L3 cache where no snoop was needed to satisfy the request. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts modified writebacks from L1 cache and L2 cache that have any type of response.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.COREWB_M.ANY_RESPONSE",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x3000000010000",
        "PublicDescription": "Counts modified writebacks from L1 cache and L2 cache that have any type of response. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts modified writebacks from L1 cache and L2 cache that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.COREWB_M.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x3001F803C0000",
        "PublicDescription": "Counts modified writebacks from L1 cache and L2 cache that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts modified writebacks from L1 cache and L2 cache that have an outstanding request. Returns the number of cycles until the response is received (i.e. XQ to XQ latency).",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.COREWB_M.OUTSTANDING",
        "MSRIndex": "0x1a6",
        "MSRValue": "0x8003000000000000",
        "PublicDescription": "Counts modified writebacks from L1 cache and L2 cache that have an outstanding request. Returns the number of cycles until the response is received (i.e. XQ to XQ latency). Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand instruction fetches and L1 instruction cache prefetches that have any type of response.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_CODE_RD.ANY_RESPONSE",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10004",
        "PublicDescription": "Counts demand instruction fetches and L1 instruction cache prefetches that have any type of response. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand instruction fetches and L1 instruction cache prefetches that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_CODE_RD.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1F803C0004",
        "PublicDescription": "Counts demand instruction fetches and L1 instruction cache prefetches that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand instruction fetches and L1 instruction cache prefetches that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_CODE_RD.L3_HIT.SNOOP_HITM",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10003C0004",
        "PublicDescription": "Counts demand instruction fetches and L1 instruction cache prefetches that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand instruction fetches and L1 instruction cache prefetches that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_CODE_RD.L3_HIT.SNOOP_HIT_NO_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x4003C0004",
        "PublicDescription": "Counts demand instruction fetches and L1 instruction cache prefetches that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand instruction fetches and L1 instruction cache prefetches that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_CODE_RD.L3_HIT.SNOOP_HIT_WITH_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x8003C0004",
        "PublicDescription": "Counts demand instruction fetches and L1 instruction cache prefetches that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand instruction fetches and L1 instruction cache prefetches that were supplied by the L3 cache where a snoop was sent but the snoop missed.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_CODE_RD.L3_HIT.SNOOP_MISS",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x2003C0004",
        "PublicDescription": "Counts demand instruction fetches and L1 instruction cache prefetches that were supplied by the L3 cache where a snoop was sent but the snoop missed. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand instruction fetches and L1 instruction cache prefetches that were supplied by the L3 cache where no snoop was needed to satisfy the request.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_CODE_RD.L3_HIT.SNOOP_NOT_NEEDED",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1003C0004",
        "PublicDescription": "Counts demand instruction fetches and L1 instruction cache prefetches that were supplied by the L3 cache where no snoop was needed to satisfy the request. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that have any type of response.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_AND_L1PF_RD.ANY_RESPONSE",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10001",
        "PublicDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that have any type of response. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1F803C0001",
        "PublicDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_HITM",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10003C0001",
        "PublicDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_HIT_NO_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x4003C0001",
        "PublicDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_HIT_WITH_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x8003C0001",
        "PublicDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that were supplied by the L3 cache where a snoop was sent but the snoop missed.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_MISS",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x2003C0001",
        "PublicDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that were supplied by the L3 cache where a snoop was sent but the snoop missed. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that were supplied by the L3 cache where no snoop was needed to satisfy the request.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_NOT_NEEDED",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1003C0001",
        "PublicDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that were supplied by the L3 cache where no snoop was needed to satisfy the request. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that have an outstanding request. Returns the number of cycles until the response is received (i.e. XQ to XQ latency).",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_AND_L1PF_RD.OUTSTANDING",
        "MSRIndex": "0x1a6",
        "MSRValue": "0x8000000000000001",
        "PublicDescription": "Counts cacheable demand data reads, L1 data cache hardware prefetches and software prefetches (except PREFETCHW) that have an outstanding request. Returns the number of cycles until the response is received (i.e. XQ to XQ latency). Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.ANY_RESPONSE",
        "Counter": "0,1,2,3",
        "Deprecated": "1",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_RD.ANY_RESPONSE",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10001",
        "PublicDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.ANY_RESPONSE Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT",
        "Counter": "0,1,2,3",
        "Deprecated": "1",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_RD.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1F803C0001",
        "PublicDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_HITM",
        "Counter": "0,1,2,3",
        "Deprecated": "1",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_RD.L3_HIT.SNOOP_HITM",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10003C0001",
        "PublicDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_HITM Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_HIT_NO_FWD",
        "Counter": "0,1,2,3",
        "Deprecated": "1",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_RD.L3_HIT.SNOOP_HIT_NO_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x4003C0001",
        "PublicDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_HIT_NO_FWD Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_HIT_WITH_FWD",
        "Counter": "0,1,2,3",
        "Deprecated": "1",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_RD.L3_HIT.SNOOP_HIT_WITH_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x8003C0001",
        "PublicDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_HIT_WITH_FWD Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_MISS",
        "Counter": "0,1,2,3",
        "Deprecated": "1",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_RD.L3_HIT.SNOOP_MISS",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x2003C0001",
        "PublicDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_MISS Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_NOT_NEEDED",
        "Counter": "0,1,2,3",
        "Deprecated": "1",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_RD.L3_HIT.SNOOP_NOT_NEEDED",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1003C0001",
        "PublicDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.L3_HIT.SNOOP_NOT_NEEDED Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.OUTSTANDING",
        "Counter": "0,1,2,3",
        "Deprecated": "1",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_DATA_RD.OUTSTANDING",
        "MSRIndex": "0x1a6",
        "MSRValue": "0x8000000000000001",
        "PublicDescription": "This event is deprecated. Refer to new event OCR.DEMAND_DATA_AND_L1PF_RD.OUTSTANDING Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that have any type of response.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_RFO.ANY_RESPONSE",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10002",
        "PublicDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that have any type of response. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_RFO.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1F803C0002",
        "PublicDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_RFO.L3_HIT.SNOOP_HITM",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10003C0002",
        "PublicDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_RFO.L3_HIT.SNOOP_HIT_NO_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x4003C0002",
        "PublicDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_RFO.L3_HIT.SNOOP_HIT_WITH_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x8003C0002",
        "PublicDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that were supplied by the L3 cache where a snoop was sent but the snoop missed.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_RFO.L3_HIT.SNOOP_MISS",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x2003C0002",
        "PublicDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that were supplied by the L3 cache where a snoop was sent but the snoop missed. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that were supplied by the L3 cache where no snoop was needed to satisfy the request.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_RFO.L3_HIT.SNOOP_NOT_NEEDED",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1003C0002",
        "PublicDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that were supplied by the L3 cache where no snoop was needed to satisfy the request. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that have an outstanding request. Returns the number of cycles until the response is received (i.e. XQ to XQ latency).",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.DEMAND_RFO.OUTSTANDING",
        "MSRIndex": "0x1a6",
        "MSRValue": "0x8000000000000002",
        "PublicDescription": "Counts demand reads for ownership (RFO) and software prefetches for exclusive ownership (PREFETCHW) that have an outstanding request. Returns the number of cycles until the response is received (i.e. XQ to XQ latency). Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts streaming stores which modify a full 64 byte cacheline that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.FULL_STREAMING_WR.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x801F803C0000",
        "PublicDescription": "Counts streaming stores which modify a full 64 byte cacheline that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L1 data cache hardware prefetches and software prefetches (except PREFETCHW and PFRFO) that have any type of response.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L1D_AND_SWPF.ANY_RESPONSE",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10400",
        "PublicDescription": "Counts L1 data cache hardware prefetches and software prefetches (except PREFETCHW and PFRFO) that have any type of response. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L1 data cache hardware prefetches and software prefetches (except PREFETCHW and PFRFO) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L1D_AND_SWPF.L3_HIT.SNOOP_HITM",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10003C0400",
        "PublicDescription": "Counts L1 data cache hardware prefetches and software prefetches (except PREFETCHW and PFRFO) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that have any type of response.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_CODE_RD.ANY_RESPONSE",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10040",
        "PublicDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that have any type of response. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_CODE_RD.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1F803C0040",
        "PublicDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_CODE_RD.L3_HIT.SNOOP_HITM",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10003C0040",
        "PublicDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_CODE_RD.L3_HIT.SNOOP_HIT_NO_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x4003C0040",
        "PublicDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_CODE_RD.L3_HIT.SNOOP_HIT_WITH_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x8003C0040",
        "PublicDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent but the snoop missed.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_CODE_RD.L3_HIT.SNOOP_MISS",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x2003C0040",
        "PublicDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent but the snoop missed. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that were supplied by the L3 cache where no snoop was needed to satisfy the request.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_CODE_RD.L3_HIT.SNOOP_NOT_NEEDED",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1003C0040",
        "PublicDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that were supplied by the L3 cache where no snoop was needed to satisfy the request. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that have an outstanding request. Returns the number of cycles until the response is received (i.e. XQ to XQ latency).",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_CODE_RD.OUTSTANDING",
        "MSRIndex": "0x1a6",
        "MSRValue": "0x8000000000000040",
        "PublicDescription": "Counts L2 cache hardware prefetch code reads (written to the L2 cache only) that have an outstanding request. Returns the number of cycles until the response is received (i.e. XQ to XQ latency). Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch data reads (written to the L2 cache only) that have any type of response.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_DATA_RD.ANY_RESPONSE",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10010",
        "PublicDescription": "Counts L2 cache hardware prefetch data reads (written to the L2 cache only) that have any type of response. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch data reads (written to the L2 cache only) that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_DATA_RD.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1F803C0010",
        "PublicDescription": "Counts L2 cache hardware prefetch data reads (written to the L2 cache only) that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch data reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_DATA_RD.L3_HIT.SNOOP_HITM",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10003C0010",
        "PublicDescription": "Counts L2 cache hardware prefetch data reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch data reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_DATA_RD.L3_HIT.SNOOP_HIT_NO_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x4003C0010",
        "PublicDescription": "Counts L2 cache hardware prefetch data reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch data reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_DATA_RD.L3_HIT.SNOOP_HIT_WITH_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x8003C0010",
        "PublicDescription": "Counts L2 cache hardware prefetch data reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch data reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent but the snoop missed.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_DATA_RD.L3_HIT.SNOOP_MISS",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x2003C0010",
        "PublicDescription": "Counts L2 cache hardware prefetch data reads (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent but the snoop missed. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch data reads (written to the L2 cache only) that were supplied by the L3 cache where no snoop was needed to satisfy the request.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_DATA_RD.L3_HIT.SNOOP_NOT_NEEDED",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1003C0010",
        "PublicDescription": "Counts L2 cache hardware prefetch data reads (written to the L2 cache only) that were supplied by the L3 cache where no snoop was needed to satisfy the request. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that have any type of response.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_RFO.ANY_RESPONSE",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10020",
        "PublicDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that have any type of response. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_RFO.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1F803C0020",
        "PublicDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_RFO.L3_HIT.SNOOP_HITM",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10003C0020",
        "PublicDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_RFO.L3_HIT.SNOOP_HIT_NO_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x4003C0020",
        "PublicDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_RFO.L3_HIT.SNOOP_HIT_WITH_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x8003C0020",
        "PublicDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent but the snoop missed.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_RFO.L3_HIT.SNOOP_MISS",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x2003C0020",
        "PublicDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that were supplied by the L3 cache where a snoop was sent but the snoop missed. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that were supplied by the L3 cache where no snoop was needed to satisfy the request.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_RFO.L3_HIT.SNOOP_NOT_NEEDED",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1003C0020",
        "PublicDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that were supplied by the L3 cache where no snoop was needed to satisfy the request. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that have an outstanding request. Returns the number of cycles until the response is received (i.e. XQ to XQ latency).",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.HWPF_L2_RFO.OUTSTANDING",
        "MSRIndex": "0x1a6",
        "MSRValue": "0x8000000000000020",
        "PublicDescription": "Counts L2 cache hardware prefetch RFOs (written to the L2 cache only) that have an outstanding request. Returns the number of cycles until the response is received (i.e. XQ to XQ latency). Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts modified writebacks from L1 cache that miss the L2 cache that have any type of response.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.L1WB_M.ANY_RESPONSE",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1000000010000",
        "PublicDescription": "Counts modified writebacks from L1 cache that miss the L2 cache that have any type of response. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts modified writebacks from L1 cache that miss the L2 cache that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.L1WB_M.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1001F803C0000",
        "PublicDescription": "Counts modified writebacks from L1 cache that miss the L2 cache that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts modified writeBacks from L2 cache that miss the L3 cache that have any type of response.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.L2WB_M.ANY_RESPONSE",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x2000000010000",
        "PublicDescription": "Counts modified writeBacks from L2 cache that miss the L3 cache that have any type of response. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts modified writeBacks from L2 cache that miss the L3 cache that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.L2WB_M.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x2001F803C0000",
        "PublicDescription": "Counts modified writeBacks from L2 cache that miss the L3 cache that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts streaming stores which modify only part of a 64 byte cacheline that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.PARTIAL_STREAMING_WR.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x401F803C0000",
        "PublicDescription": "Counts streaming stores which modify only part of a 64 byte cacheline that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that have any type of response.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.READS_TO_CORE.ANY_RESPONSE",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10477",
        "PublicDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that have any type of response. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.READS_TO_CORE.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1F803C0477",
        "PublicDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.READS_TO_CORE.L3_HIT.SNOOP_HITM",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x10003C0477",
        "PublicDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.READS_TO_CORE.L3_HIT.SNOOP_HIT_NO_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x4003C0477",
        "PublicDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.READS_TO_CORE.L3_HIT.SNOOP_HIT_WITH_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x8003C0477",
        "PublicDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that were supplied by the L3 cache where a snoop was sent but the snoop missed.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.READS_TO_CORE.L3_HIT.SNOOP_MISS",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x2003C0477",
        "PublicDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that were supplied by the L3 cache where a snoop was sent but the snoop missed. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that were supplied by the L3 cache where no snoop was needed to satisfy the request.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.READS_TO_CORE.L3_HIT.SNOOP_NOT_NEEDED",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1003C0477",
        "PublicDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that were supplied by the L3 cache where no snoop was needed to satisfy the request. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that have an outstanding request. Returns the number of cycles until the response is received (i.e. XQ to XQ latency).",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.READS_TO_CORE.OUTSTANDING",
        "MSRIndex": "0x1a6",
        "MSRValue": "0x8000000000000477",
        "PublicDescription": "Counts all data read, code read and RFO requests including demands and prefetches to the core caches (L1 or L2) that have an outstanding request. Returns the number of cycles until the response is received (i.e. XQ to XQ latency). Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts streaming stores that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.STREAMING_WR.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1F803C0800",
        "PublicDescription": "Counts streaming stores that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts uncached memory reads that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.UC_RD.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x101F803C0000",
        "PublicDescription": "Counts uncached memory reads that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts uncached memory reads that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.UC_RD.L3_HIT.SNOOP_HITM",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1010003C0000",
        "PublicDescription": "Counts uncached memory reads that were supplied by the L3 cache where a snoop was sent, the snoop hit, and modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts uncached memory reads that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.UC_RD.L3_HIT.SNOOP_HIT_NO_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1004003C0000",
        "PublicDescription": "Counts uncached memory reads that were supplied by the L3 cache where a snoop was sent, the snoop hit, but no data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts uncached memory reads that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.UC_RD.L3_HIT.SNOOP_HIT_WITH_FWD",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1008003C0000",
        "PublicDescription": "Counts uncached memory reads that were supplied by the L3 cache where a snoop was sent, the snoop hit, and non-modified data was forwarded. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts uncached memory reads that were supplied by the L3 cache where a snoop was sent but the snoop missed.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.UC_RD.L3_HIT.SNOOP_MISS",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1002003C0000",
        "PublicDescription": "Counts uncached memory reads that were supplied by the L3 cache where a snoop was sent but the snoop missed. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts uncached memory reads that were supplied by the L3 cache where no snoop was needed to satisfy the request.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.UC_RD.L3_HIT.SNOOP_NOT_NEEDED",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x1001003C0000",
        "PublicDescription": "Counts uncached memory reads that were supplied by the L3 cache where no snoop was needed to satisfy the request. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts uncached memory writes that were supplied by the L3 cache.",
        "Counter": "0,1,2,3",
        "EventCode": "0XB7",
        "EventName": "OCR.UC_WR.L3_HIT",
        "MSRIndex": "0x1a6,0x1a7",
        "MSRValue": "0x201F803C0000",
        "PublicDescription": "Counts uncached memory writes that were supplied by the L3 cache. Available PDIST counters: 0",
        "SampleAfterValue": "100003",
        "UMask": "0x1"
    },
    {
        "BriefDescription": "Counts the number of issue slots every cycle that were not delivered by the frontend due to instruction cache misses.",
        "Counter": "0,1,2,3",
        "EventCode": "0x71",
        "EventName": "TOPDOWN_FE_BOUND.ICACHE",
        "SampleAfterValue": "1000003",
        "UMask": "0x20"
    }
]
