[
  {
    "content": "Check current build status and verify kernel/initramfs artifacts",
    "status": "completed",
    "priority": "high",
    "id": "todo_1"
  },
  {
    "content": "Build proper initramfs with s390x-compatible busybox",
    "status": "completed",
    "priority": "high",
    "id": "todo_2"
  },
  {
    "content": "Fix mkinitcpio missing dependencies: busybox, blkid, switch_root, libkmod, bsdtar",
    "status": "completed",
    "priority": "high",
    "id": "todo_3"
  },
  {
    "content": "Prepare boot files and configuration",
    "status": "completed",
    "priority": "high",
    "id": "todo_4"
  },
  {
    "content": "Test booting with QEMU s390x emulation",
    "status": "completed",
    "priority": "medium",
    "id": "todo_5"
  },
  {
    "content": "Create minimal s390x root filesystem",
    "status": "completed",
    "priority": "high",
    "id": "todo_6"
  },
  {
    "content": "Cross-compile s390x busybox for root filesystem",
    "status": "completed",
    "priority": "high",
    "id": "todo_7"
  },
  {
    "content": "Create working init system using initramfs only",
    "status": "completed",
    "priority": "high",
    "id": "todo_8"
  },
  {
    "content": "Document the successful s390x Arch Linux port",
    "status": "completed",
    "priority": "low",
    "id": "todo_9"
  }
]