default
xkb_keycodes "jolla" {

   // These keycodes are beyond the X11 255 limit value so it would
   // only be valid for the use with SW which supports extended keycodes,
   // like xkbcommon.

   <I264> = 264;	// Jolla phone has the wired headset button sending this keycode

};
