+	if (!adcx140->gpio_reset)
 		dev_info(&i2c->dev, "Reset GPIO not defined\n");
 
 	adcx140->supply_areg = devm_regulator_get_optional(adcx140->dev,
-- 
2.51.0[PATCH 5.10 18/41] ASoC: tlv320adcx140: Propagate error codes during probeGreg Kroah-Hartman <gregkh@linuxfoundation.org> undefinedstable@vger.kernel.org undefined undefined undefined undefined undefined undefined‘I…î