or output image

    Returns:
        PIL Image: Grayscale version of the input.

        - If ``num_output_channels == 1`` : returned image is single channel
        - If ``num_output_channels == 3`` : returned image is 3 channel with r == g == b

    r