` returns an array giving the frequencies
of corresponding elements in the output.  The routine
``np.fft.fftshift(A)`` shifts transforms and their frequencies to put the
zero-frequency components in the middle, and ``np.fft.ifftshift(A)`` undoes
that shift.

When the input `a` is a time-domain signal and ``A = fft(a)``, ``np.abs(A)``
is its amplitude spectrum and ``np.abs(A)**2`` is its power spectrum.
The phase spectrum is obtained by ``np.angle(A)``.

The inverse DFT is defined as

.. math::
   a_m = \frac{1}{n}\sum_{k=0}^{n-1}A_k\exp\left\{2\pi i{mk\over n}\right\}
   \qquad m = 0,\ldots,n-1.

It differs from the forward transform by the sign of the exponential
argument and the default normalization by :math:`1/n`.

Type Promotion
--------------

`numpy.fft` promotes ``float32`` and ``complex64`` arrays to ``float64`` and
``complex128`` arrays respectively. For an FFT implementation that does not
promote input arrays, see `scipy.fftpack`.

Normalization
-------------

The argument ``norm`` indicates which direction of the pair of direct/inverse
transforms is scaled and with what normalization factor.
The default normalization (``"backward"``) has the direct (forward) transforms
unscaled and the inverse (backward) transforms scaled by :math:`1/n`. It is
possible to obtain unitary transforms by setting the keyword argument ``norm``
to ``"ortho"`` so that both direct and inverse transforms are scaled by
:math:`1/\sqrt{n}`. Finally, setting the keyword argument ``norm`` to
``"forward"`` has the direct transforms scaled by :math:`1/n` and the inverse
transforms unscaled (i.e. exactly opposite to the default ``"backward"``).
`None` is an alias of the default option ``"backward"`` for backward
compatibility.

Real and Hermitian transforms
-----------------------------

When the input is purely real, its transform is Hermitian, i.e., the
component at frequency :math:`f_k` is the complex conjugate of the
component at frequency :math:`-f_k`, which means that for real
inputs there is no information in the negative frequency components that
is not already available from the positive frequency components.
The family of `rfft` functions is
designed to operate on real inputs, and exploits this symmetry by
computing only the positive frequency components, up to and including the
Nyquist frequency.  Thus, ``n`` input points produce ``n/2+1`` complex
output points.  The inverses of this family assumes the same symmetry of
its input, and for an output of ``n`` points uses ``n/2+1`` input points.

Correspondingly, when the spectrum is purely real, the signal is
Hermitian.  The `hfft` family of functions exploits this symmetry by
using ``n/2+1`` complex points in the input (time) domain for ``n`` real
points in the frequency domain.

In higher dimensions, FFTs are used, e.g., for image analysis and
filtering.  The computational efficiency of the FFT means that it can
also be a faster way to compute large convolutions, using the property
that a convolution in the time domain is equivalent to a point-by-point
multiplication in the frequency domain.

Higher dimensions
-----------------

In two dimensions, the DFT is defined as

.. math::
   A_{kl} =  \sum_{m=0}^{M-1} \sum_{n=0}^{N-1}
   a_{mn}\exp\left\{-2\pi i \left({mk\over M}+{nl\over N}\right)\right\}
   \qquad k = 0, \ldots, M-1;\quad l = 0, \ldots, N-1,

which extends in the obvious way to higher dimensions, and the inverses
in higher dimensions also extend in the same way.

References
----------

.. [CT] Cooley, James W., and John W. Tukey, 1965, "An algorithm for the
        machine calculation of complex Fourier series," *Math. Comput.*
        19: 297-301.

.. [NR] Press, W., Teukolsky, S., Vetterline, W.T., and Flannery, B.P.,
        2007, *Numerical Recipes: The Art of Scientific Computing*, ch.
        12-13.  Cambridge Univ. Press, Cambridge, UK.

Examples
--------

For examples, see the various functions.

