{
  "schema_version": "1.4.0",
  "id": "GHSA-79jh-4xm7-4v3x",
  "modified": "2022-05-14T01:31:02Z",
  "published": "2022-05-14T01:31:02Z",
  "aliases": [
    "CVE-2019-9111"
  ],
  "details": "The msm gpu driver for custom Linux kernels on the Xiaomi perseus-p-oss MIX 3 device through 2018-11-26 has an integer overflow and OOPS because of missing checks of the count argument in sde_evtlog_filter_write in drivers/gpu/drm/msm/sde_dbg.c. This is exploitable for a device crash via a syscall by a crafted application on a rooted device.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:L/AC:L/PR:N/UI:R/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2019-9111"
    },
    {
      "type": "WEB",
      "url": "https://github.com/MiCode/Xiaomi_Kernel_OpenSource/issues/1001"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-190"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2019-02-25T04:29:00Z"
  }
}