{
  "schema_version": "1.4.0",
  "id": "GHSA-7c6h-cf9x-293j",
  "modified": "2022-05-24T22:00:15Z",
  "published": "2022-05-24T22:00:15Z",
  "aliases": [
    "CVE-2019-2292"
  ],
  "details": "Out of bound access can occur due to buffer copy without checking size of input received from WLAN firmware in Snapdragon Auto, Snapdragon Consumer IOT, Snapdragon Industrial IOT, Snapdragon Mobile, Snapdragon Voice & Music in MDM9150, MDM9650, MSM8996AU, QCA6574AU, QCS405, QCS605, SD 210/SD 212/SD 205, SD 425, SD 427, SD 430, SD 435, SD 450, SD 625, SD 636, SD 665, SD 712 / SD 710 / SD 670, SD 730, SD 820A, SD 835, SD 845 / SD 850, SD 855, SDA660, SDM630, SDM660, SDX20, SDX24",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2019-2292"
    },
    {
      "type": "WEB",
      "url": "https://www.codeaurora.org/security-bulletin/2019/06/03/june-2019-code-aurora-security-bulletin"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2019-07-22T14:15:00Z"
  }
}