{
  "schema_version": "1.4.0",
  "id": "GHSA-7h55-hg3x-w6vg",
  "modified": "2022-05-14T03:28:11Z",
  "published": "2022-05-14T03:28:11Z",
  "aliases": [
    "CVE-2016-10464"
  ],
  "details": "In Android before 2018-04-05 or earlier security patch level on Qualcomm Snapdragon Mobile and Snapdragon Wear MDM9206, MDM9607, MDM9640, MDM9650, QCA6174A, QCA6574AU, QCA9377, SD 210/SD 212/SD 205, SD 425, SD 600, SD 650/52, SD 808, SD 810, SD 820, and SDX20, lack of input validation for HCI H4 UART packet ID cause system denial of service.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2016-10464"
    },
    {
      "type": "WEB",
      "url": "https://source.android.com/security/bulletin/2018-04-01"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/103671"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-20"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-04-18T14:29:00Z"
  }
}