{
  "schema_version": "1.4.0",
  "id": "GHSA-7gv3-h552-264c",
  "modified": "2022-05-17T05:13:14Z",
  "published": "2022-05-17T05:13:14Z",
  "aliases": [
    "CVE-2012-3063"
  ],
  "details": "Cisco Application Control Engine (ACE) before A4(2.3) and A5 before A5(1.1), when multicontext mode is enabled, does not properly share a management IP address among multiple contexts, which allows remote authenticated administrators to bypass intended access restrictions in opportunistic circumstances, and read or modify configuration settings, via a login attempt to a context, aka Bug ID CSCts30631, a different vulnerability than CVE-2012-3058.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2012-3063"
    },
    {
      "type": "WEB",
      "url": "http://tools.cisco.com/security/center/content/CiscoSecurityAdvisory/cisco-sa-20120620-ace"
    },
    {
      "type": "WEB",
      "url": "http://www.securitytracker.com/id?1027188"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-362"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2012-06-20T20:55:00Z"
  }
}