{
  "schema_version": "1.4.0",
  "id": "GHSA-7gg9-xr98-9cmr",
  "modified": "2022-05-13T01:44:01Z",
  "published": "2022-05-13T01:44:01Z",
  "aliases": [
    "CVE-2017-15845"
  ],
  "details": "In Android for MSM, Firefox OS for MSM, QRD Android, with all Android releases from CAF using the Linux kernel, an invalid input of firmware size (negative value) from user space can potentially lead to the memory leak or buffer overflow during the WLAN cal data store operation.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:L/AC:L/PR:L/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2017-15845"
    },
    {
      "type": "WEB",
      "url": "https://source.android.com/security/bulletin/pixel/2018-01-01"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-20"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-01-10T22:29:00Z"
  }
}