{
  "schema_version": "1.4.0",
  "id": "GHSA-7h7m-5mrv-qfq7",
  "modified": "2022-05-24T17:40:36Z",
  "published": "2022-05-24T17:40:36Z",
  "aliases": [
    "CVE-2021-25127"
  ],
  "details": "The Baseboard Management Controller(BMC) in HPE Cloudline CL5800 Gen9 Server; HPE Cloudline CL5200 Gen9 Server; HPE Cloudline CL4100 Gen10 Server; HPE Cloudline CL3100 Gen10 Server; HPE Cloudline CL5800 Gen10 Server BMC firmware has a local buffer overlfow in spx_restservice generatesslcertificate_func function.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2021-25127"
    },
    {
      "type": "WEB",
      "url": "https://support.hpe.com/hpsc/doc/public/display?docLocale=en_US&docId=emr_na-hpesbhf04073en_us"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-120"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2021-01-29T19:15:00Z"
  }
}