{
  "schema_version": "1.4.0",
  "id": "GHSA-5m6q-c52m-c8v4",
  "modified": "2025-09-29T21:30:20Z",
  "published": "2025-09-29T21:30:20Z",
  "aliases": [
    "CVE-2025-56752"
  ],
  "details": "A vulnerability in the Ruijie RG-ES series switch firmware ESW_1.0(1)B1P39 enables remote attackers to fully bypass authentication mechanisms, providing them with unrestricted access to alter administrative settings and potentially seize control of affected devices via crafted HTTP POST request to /user.cgi.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:N/AC:L/PR:N/UI:N/S:U/C:H/I:L/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2025-56752"
    },
    {
      "type": "WEB",
      "url": "https://github.com/TNCX-byte/Vulnerability_Research/blob/main/CVE-2025-56752/README.md"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-287"
    ],
    "severity": "CRITICAL",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2025-09-03T18:15:35Z"
  }
}