{
  "schema_version": "1.4.0",
  "id": "GHSA-4x6r-qc3x-j39x",
  "modified": "2025-09-15T09:30:19Z",
  "published": "2025-09-15T09:30:19Z",
  "aliases": [
    "CVE-2025-41713"
  ],
  "details": "During a short time frame while the device is booting an unauthenticated remote attacker can send traffic to unauthorized networks due to the switch operating in an undefined state until a CPU-induced reset allows proper configuration.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:N/AC:L/PR:N/UI:N/S:U/C:L/I:N/A:L"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2025-41713"
    },
    {
      "type": "WEB",
      "url": "https://certvde.com/en/advisories/VDE-2025-083"
    },
    {
      "type": "WEB",
      "url": "https://wago.csaf-tp.certvde.com/.well-known/csaf/white/2025/vde-2025-083.json"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-1188"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2025-09-15T08:15:35Z"
  }
}