apiVersion: apiextensions.k8s.io/v1
kind: CustomResourceDefinition
metadata:
  annotations:
    api-approved.openshift.io: https://github.com/openshift/api/pull/475
    include.release.openshift.io/self-managed-high-availability: "true"
    include.release.openshift.io/single-node-developer: "true"
  name: networks.operator.openshift.io
spec:
  group: operator.openshift.io
  names:
    kind: Network
    listKind: NetworkList
    plural: networks
    singular: network
  scope: Cluster
  versions:
  - name: v1
    schema:
      openAPIV3Schema:
        description: "Network describes the cluster's desired network configuration.
          It is consumed by the cluster-network-operator. \n Compatibility level 1:
          Stable within a major release for a minimum of 12 months or 3 minor releases
          (whichever is longer)."
        properties:
          apiVersion:
            description: 'APIVersion defines the versioned schema of this representation
              of an object. Servers should convert recognized schemas to the latest
              internal value, and may reject unrecognized values. More info: https://git.k8s.io/community/contributors/devel/sig-architecture/api-conventions.md#resources'
            type: string
          kind:
            description: 'Kind is a string value representing the REST resource this
              object represents. Servers may infer this from the endpoint the client
              submits requests to. Cannot be updated. In CamelCase. More info: https://git.k8s.io/community/contributors/devel/sig-architecture/api-conventions.md#types-kinds'
            type: string
          metadata:
            type: object
          spec:
            description: NetworkSpec is the top-level network configuration object.
            properties:
              additionalNetworks:
                description: additionalNetworks is a list of extra networks to make
                  available to pods when multiple networks are enabled.
                items:
                  description: AdditionalNetworkDefinition configures an extra network
                    that is available but not created by default. Instead, pods must
                    request them by name. type must be specified, along with exactly
                    one "Config" that matches the type.
                  properties:
                    name:
                      description: name is the name of the network. This will be populated
                        in the resulting CRD This must be unique.
                      type: string
                    namespace:
                      description: namespace is the namespace of the network. This
                        will be populated in the resulting CRD If not given the network
                        will be created in the default namespace.
                      type: string
                    rawCNIConfig:
                      description: rawCNIConfig is the raw CNI configuration json
                        to create in the NetworkAttachmentDefinition CRD
                      type: string
                    simpleMacvlanConfig:
                      description: SimpleMacvlanConfig configures the macvlan interface
                        in case of type:NetworkTypeSimpleMacvlan
                      properties:
                        ipamConfig:
                          description: IPAMConfig configures IPAM module will be used
                            for IP Address Management (IPAM).
                          properties:
                            staticIPAMConfig:
                              description: StaticIPAMConfig configures the static
                                IP address in case of type:IPAMTypeStatic
                              properties:
                                addresses:
                                  description: Addresses configures IP address for
                                    the interface
                                  items:
                                    description: StaticIPAMAddresses provides IP address
                                      and Gateway for static IPAM addresses
                                    properties:
                                      address:
                                        description: Address is the IP address in
                                          CIDR format
                                        type: string
                                      gateway:
                                        description: Gateway is IP inside of subnet
                                          to designate as the gateway
                                        type: string
                                    type: object
                                  type: array
                                dns:
                                  description: DNS configures DNS for the interface
                                  properties:
                                    domain:
                                      description: Domain configures the domainname
                                        the local domain used for short hostname lookups
                                      type: string
                                    nameservers:
                                      description: Nameservers points DNS servers
                                        for IP lookup
                                      items:
                                        type: string
                                      type: array
                                    search:
                                      description: Search configures priority ordered
                                        search domains for short hostname lookups
                                      items:
                                        type: string
                                      type: array
                                  type: object
                                routes:
                                  description: Routes configures IP routes for the
                                    interface
                                  items:
                                    description: StaticIPAMRoutes provides Destination/Gateway
                                      pairs for static IPAM routes
                                    properties:
                                      destination:
                                        description: Destination points the IP route
                                          destination
                                        type: string
                                      gateway:
                                        description: Gateway is the route's next-hop
                                          IP address If unset, a default gateway is
                                          assumed (as determined by the CNI plugin).
                                        type: string
                                    type: object
                                  type: array
                              type: object
                            type:
                              description: Type is the type of IPAM module will be
                                used for IP Address Management(IPAM). The supported
                                values are IPAMTypeDHCP, IPAMTypeStatic
                              type: string
                          type: object
                        master:
                          description: master is the host interface to create the
                            macvlan interface from. If not specified, it will be default
                            route interface
                          type: string
                        mode:
                          description: 'mode is the macvlan mode: bridge, private,
                            vepa, passthru. The default is bridge'
                          type: string
                        mtu:
                          description: mtu is the mtu to use for the macvlan interface.
                            if unset, host's kernel will select the value.
                          format: int32
                          minimum: 0
                          type: integer
                      type: object
                    type:
                      description: type is the type of network The supported values
                        are NetworkTypeRaw, NetworkTypeSimpleMacvlan
                      type: string
                  type: object
                type: array
              clusterNetwork:
                description: clusterNetwork is the IP address pool to use for pod
                  IPs. Some network providers, e.g. OpenShift SDN, support multiple
                  ClusterNetworks. Others only support one. This is equivalent to
                  the cluster-cidr.
                items:
                  description: ClusterNetworkEntry is a subnet from which to allocate
                    PodIPs. A network of size HostPrefix (in CIDR notation) will be
                    allocated when nodes join the cluster. If the HostPrefix field
                    is not used by the plugin, it can be left unset. Not all network
                    providers support multiple ClusterNetworks
                  properties:
                    cidr:
                      type: string
                    hostPrefix:
                      format: int32
                      minimum: 0
                      type: integer
                  type: object
                type: array
              defaultNetwork:
                description: defaultNetwork is the "default" network that all pods
                  will receive
                properties:
                  kuryrConfig:
                    description: KuryrConfig configures the kuryr plugin
                    properties:
                      controllerProbesPort:
                        description: The port kuryr-controller will listen for readiness
                          and liveness requests.
                        format: int32
                        minimum: 0
                        type: integer
                      daemonProbesPort:
                        description: The port kuryr-daemon will listen for readiness
                          and liveness requests.
                        format: int32
                        minimum: 0
                        type: integer
                      enablePortPoolsPrepopulation:
                        description: enablePortPoolsPrepopulation when true will make
                          Kuryr prepopulate each newly created port pool with a minimum
                          number of ports. Kuryr uses Neutron port pooling to fight
                          the fact that it takes a significant amount of time to create
                          one. It creates a number of ports when the first pod that
                          is configured to use the dedicated network for pods is created
                          in a namespace, and keeps them ready to be attached to pods.
                          Port prepopulation is disabled by default.
                        type: boolean
                      mtu:
                        description: mtu is the MTU that Kuryr should use when creating
                          pod networks in Neutron. The value has to be lower or equal
                          to the MTU of the nodes network and Neutron has to allow
                          creation of tenant networks with such MTU. If unset Pod
                          networks will be created with the same MTU as the nodes
                          network has.
                        format: int32
                        minimum: 0
                        type: integer
                      openStackServiceNetwork:
                        description: openStackServiceNetwork contains the CIDR of
                          network from which to allocate IPs for OpenStack Octavia's
                          Amphora VMs. Please note that with Amphora driver Octavia
                          uses two IPs from that network for each loadbalancer - one
                          given by OpenShift and second for VRRP connections. As the
                          first one is managed by OpenShift's and second by Neutron's
                          IPAMs, those need to come from different pools. Therefore
                          `openStackServiceNetwork` needs to be at least twice the
                          size of `serviceNetwork`, and whole `serviceNetwork` must
                          be overlapping with `openStackServiceNetwork`. cluster-network-operator
                          will then make sure VRRP IPs are taken from the ranges inside
                          `openStackServiceNetwork` that are not overlapping with
                          `serviceNetwork`, effectivly preventing conflicts. If not
                          set cluster-network-operator will use `serviceNetwork` expanded
                          by decrementing the prefix size by 1.
                        type: string
                      poolBatchPorts:
                        description: poolBatchPorts sets a number of ports that should
                          be created in a single batch request to extend the port
                          pool. The default is 3. For more information about port
                          pools see enablePortPoolsPrepopulation setting.
                        minimum: 0
                        type: integer
                      poolMaxPorts:
                        description: poolMaxPorts sets a maximum number of free ports
                          that are being kept in a port pool. If the number of ports
                          exceeds this setting, free ports will get deleted. Setting
                          0 will disable this upper bound, effectively preventing
                          pools from shrinking and this is the default value. For
                          more information about port pools see enablePortPoolsPrepopulation
                          setting.
                        minimum: 0
                        type: integer
                      poolMinPorts:
                        description: poolMinPorts sets a minimum number of free ports
                          that should be kept in a port pool. If the number of ports
                          is lower than this setting, new ports will get created and
                          added to pool. The default is 1. For more information about
                          port pools see enablePortPoolsPrepopulation setting.
                        minimum: 1
                        type: integer
                    type: object
                  openshiftSDNConfig:
                    description: openShiftSDNConfig configures the openshift-sdn plugin
                    properties:
                      enableUnidling:
                        description: enableUnidling controls whether or not the service
                          proxy will support idling and unidling of services. By default,
                          unidling is enabled.
                        type: boolean
                      mode:
                        description: mode is one of "Multitenant", "Subnet", or "NetworkPolicy"
                        type: string
                      mtu:
                        description: mtu is the mtu to use for the tunnel interface.
                          Defaults to 1450 if unset. This must be 50 bytes smaller
                          than the machine's uplink.
                        format: int32
                        minimum: 0
                        type: integer
                      useExternalOpenvswitch:
                        description: 'useExternalOpenvswitch used to control whether
                          the operator would deploy an OVS DaemonSet itself or expect
                          someone else to start OVS. As of 4.6, OVS is always run
                          as a system service, and this flag is ignored. DEPRECATED:
                          non-functional as of 4.6'
                        type: boolean
                      vxlanPort:
                        description: vxlanPort is the port to use for all vxlan packets.
                          The default is 4789.
                        format: int32
                        minimum: 0
                        type: integer
                    type: object
                  ovnKubernetesConfig:
                    description: ovnKubernetesConfig configures the ovn-kubernetes
                      plugin.
                    properties:
                      egressIPConfig:
                        description: egressIPConfig holds the configuration for EgressIP
                          options.
                        properties:
                          reachabilityTotalTimeoutSeconds:
                            description: reachabilityTotalTimeout configures the EgressIP
                              node reachability check total timeout in seconds. If
                              the EgressIP node cannot be reached within this timeout,
                              the node is declared down. Setting a large value may
                              cause the EgressIP feature to react slowly to node changes.
                              In particular, it may react slowly for EgressIP nodes
                              that really have a genuine problem and are unreachable.
                              When omitted, this means the user has no opinion and
                              the platform is left to choose a reasonable default,
                              which is subject to change over time. The current default
                              is 1 second. A value of 0 disables the EgressIP node's
                              reachability check.
                            format: int32
                            maximum: 60
                            minimum: 0
                            type: integer
                        type: object
                      gatewayConfig:
                        description: gatewayConfig holds the configuration for node
                          gateway options.
                        properties:
                          routingViaHost:
                            default: false
                            description: RoutingViaHost allows pod egress traffic
                              to exit via the ovn-k8s-mp0 management port into the
                              host before sending it out. If this is not set, traffic
                              will always egress directly from OVN to outside without
                              touching the host stack. Setting this to true means
                              hardware offload will not be supported. Default is false
                              if GatewayConfig is specified.
                            type: boolean
                        type: object
                      genevePort:
                        description: geneve port is the UDP port to be used by geneve
                          encapulation. Default is 6081
                        format: int32
                        minimum: 1
                        type: integer
                      hybridOverlayConfig:
                        description: HybridOverlayConfig configures an additional
                          overlay network for peers that are not using OVN.
                        properties:
                          hybridClusterNetwork:
                            description: HybridClusterNetwork defines a network space
                              given to nodes on an additional overlay network.
                            items:
                              description: ClusterNetworkEntry is a subnet from which
                                to allocate PodIPs. A network of size HostPrefix (in
                                CIDR notation) will be allocated when nodes join the
                                cluster. If the HostPrefix field is not used by the
                                plugin, it can be left unset. Not all network providers
                                support multiple ClusterNetworks
                              properties:
                                cidr:
                                  type: string
                                hostPrefix:
                                  format: int32
                                  minimum: 0
                                  type: integer
                              type: object
                            type: array
                          hybridOverlayVXLANPort:
                            description: HybridOverlayVXLANPort defines the VXLAN
                              port number to be used by the additional overlay network.
                              Default is 4789
                            format: int32
                            type: integer
                        type: object
                      ipsecConfig:
                        description: ipsecConfig enables and configures IPsec for
                          pods on the pod network within the cluster.
                        type: object
                      mtu:
                        description: mtu is the MTU to use for the tunnel interface.
                          This must be 100 bytes smaller than the uplink mtu. Default
                          is 1400
                        format: int32
                        minimum: 0
                        type: integer
                      policyAuditConfig:
                        description: policyAuditConfig is the configuration for network
                          policy audit events. If unset, reported defaults are used.
                        properties:
                          destination:
                            default: "null"
                            description: 'destination is the location for policy log
                              messages. Regardless of this config, persistent logs
                              will always be dumped to the host at /var/log/ovn/ however
                              Additionally syslog output may be configured as follows.
                              Valid values are: - "libc" -> to use the libc syslog()
                              function of the host node''s journdald process - "udp:host:port"
                              -> for sending syslog over UDP - "unix:file" -> for
                              using the UNIX domain socket directly - "null" -> to
                              discard all messages logged to syslog The default is
                              "null"'
                            type: string
                          maxFileSize:
                            default: 50
                            description: maxFilesSize is the max size an ACL_audit
                              log file is allowed to reach before rotation occurs
                              Units are in MB and the Default is 50MB
                            format: int32
                            minimum: 1
                            type: integer
                          rateLimit:
                            default: 20
                            description: rateLimit is the approximate maximum number
                              of messages to generate per-second per-node. If unset
                              the default of 20 msg/sec is used.
                            format: int32
                            minimum: 1
                            type: integer
                          syslogFacility:
                            default: local0
                            description: syslogFacility the RFC5424 facility for generated
                              messages, e.g. "kern". Default is "local0"
                            type: string
                        type: object
                      v4InternalSubnet:
                        description: v4InternalSubnet is a v4 subnet used internally
                          by ovn-kubernetes in case the default one is being already
                          used by something else. It must not overlap with any other
                          subnet being used by OpenShift or by the node network. The
                          size of the subnet must be larger than the number of nodes.
                          The value cannot be changed after installation. Default
                          is 100.64.0.0/16
                        type: string
                      v6InternalSubnet:
                        description: v6InternalSubnet is a v6 subnet used internally
                          by ovn-kubernetes in case the default one is being already
                          used by something else. It must not overlap with any other
                          subnet being used by OpenShift or by the node network. The
                          size of the subnet must be larger than the number of nodes.
                          The value cannot be changed after installation. Default
                          is fd98::/48
                        type: string
                    type: object
                  type:
                    description: type is the type of network All NetworkTypes are
                      supported except for NetworkTypeRaw
                    type: string
                type: object
              deployKubeProxy:
                description: deployKubeProxy specifies whether or not a standalone
                  kube-proxy should be deployed by the operator. Some network providers
                  include kube-proxy or similar functionality. If unset, the plugin
                  will attempt to select the correct value, which is false when OpenShift
                  SDN and ovn-kubernetes are used and true otherwise.
                type: boolean
              disableMultiNetwork:
                description: disableMultiNetwork specifies whether or not multiple
                  pod network support should be disabled. If unset, this property
                  defaults to 'false' and multiple network support is enabled.
                type: boolean
              disableNetworkDiagnostics:
                default: false
                description: disableNetworkDiagnostics specifies whether or not PodNetworkConnectivityCheck
                  CRs from a test pod to every node, apiserver and LB should be disabled
                  or not. If unset, this property defaults to 'false' and network
                  diagnostics is enabled. Setting this to 'true' would reduce the
                  additional load of the pods performing the checks.
                type: boolean
              exportNetworkFlows:
                description: exportNetworkFlows enables and configures the export
                  of network flow metadata from the pod network by using protocols
                  NetFlow, SFlow or IPFIX. Currently only supported on OVN-Kubernetes
                  plugin. If unset, flows will not be exported to any collector.
                properties:
                  ipfix:
                    description: ipfix defines IPFIX configuration.
                    properties:
                      collectors:
                        description: ipfixCollectors is list of strings formatted
                          as ip:port with a maximum of ten items
                        items:
                          pattern: ^(([0-9]|[0-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5])\.){3}([0-9]|[0-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5]):([1-9][0-9]{0,3}|[1-5][0-9]{4}|6[0-4][0-9]{3}|65[0-4][0-9]{2}|655[0-2][0-9]|6553[0-5])$
                          type: string
                        maxItems: 10
                        minItems: 1
                        type: array
                    type: object
                  netFlow:
                    description: netFlow defines the NetFlow configuration.
                    properties:
                      collectors:
                        description: netFlow defines the NetFlow collectors that will
                          consume the flow data exported from OVS. It is a list of
                          strings formatted as ip:port with a maximum of ten items
                        items:
                          pattern: ^(([0-9]|[0-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5])\.){3}([0-9]|[0-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5]):([1-9][0-9]{0,3}|[1-5][0-9]{4}|6[0-4][0-9]{3}|65[0-4][0-9]{2}|655[0-2][0-9]|6553[0-5])$
                          type: string
                        maxItems: 10
                        minItems: 1
                        type: array
                    type: object
                  sFlow:
                    description: sFlow defines the SFlow configuration.
                    properties:
                      collectors:
                        description: sFlowCollectors is list of strings formatted
                          as ip:port with a maximum of ten items
                        items:
                          pattern: ^(([0-9]|[0-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5])\.){3}([0-9]|[0-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5]):([1-9][0-9]{0,3}|[1-5][0-9]{4}|6[0-4][0-9]{3}|65[0-4][0-9]{2}|655[0-2][0-9]|6553[0-5])$
                          type: string
                        maxItems: 10
                        minItems: 1
                        type: array
                    type: object
                type: object
              kubeProxyConfig:
                description: kubeProxyConfig lets us configure desired proxy configuration.
                  If not specified, sensible defaults will be chosen by OpenShift
                  directly. Not consumed by all network providers - currently only
                  openshift-sdn.
                properties:
                  bindAddress:
                    description: The address to "bind" on Defaults to 0.0.0.0
                    type: string
                  iptablesSyncPeriod:
                    description: 'An internal kube-proxy parameter. In older releases
                      of OCP, this sometimes needed to be adjusted in large clusters
                      for performance reasons, but this is no longer necessary, and
                      there is no reason to change this from the default value. Default:
                      30s'
                    type: string
                  proxyArguments:
                    additionalProperties:
                      description: ProxyArgumentList is a list of arguments to pass
                        to the kubeproxy process
                      items:
                        type: string
                      type: array
                    description: Any additional arguments to pass to the kubeproxy
                      process
                    type: object
                type: object
              logLevel:
                default: Normal
                description: "logLevel is an intent based logging for an overall component.
                  \ It does not give fine grained control, but it is a simple way
                  to manage coarse grained logging choices that operators have to
                  interpret for their operands. \n Valid values are: \"Normal\", \"Debug\",
                  \"Trace\", \"TraceAll\". Defaults to \"Normal\"."
                enum:
                - ""
                - Normal
                - Debug
                - Trace
                - TraceAll
                type: string
              managementState:
                description: managementState indicates whether and how the operator
                  should manage the component
                pattern: ^(Managed|Unmanaged|Force|Removed)$
                type: string
              migration:
                description: migration enables and configures the cluster network
                  migration. The migration procedure allows to change the network
                  type and the MTU.
                properties:
                  features:
                    description: features contains the features migration configuration.
                      Set this to migrate feature configuration when changing the
                      cluster default network provider. if unset, the default operation
                      is to migrate all the configuration of supported features.
                    properties:
                      egressFirewall:
                        default: true
                        description: egressFirewall specifies whether or not the Egress
                          Firewall configuration is migrated automatically when changing
                          the cluster default network provider. If unset, this property
                          defaults to 'true' and Egress Firewall configure is migrated.
                        type: boolean
                      egressIP:
                        default: true
                        description: egressIP specifies whether or not the Egress
                          IP configuration is migrated automatically when changing
                          the cluster default network provider. If unset, this property
                          defaults to 'true' and Egress IP configure is migrated.
                        type: boolean
                      multicast:
                        default: true
                        description: multicast specifies whether or not the multicast
                          configuration is migrated automatically when changing the
                          cluster default network provider. If unset, this property
                          defaults to 'true' and multicast configure is migrated.
                        type: boolean
                    type: object
                  mtu:
                    description: mtu contains the MTU migration configuration. Set
                      this to allow changing the MTU values for the default network.
                      If unset, the operation of changing the MTU for the default
                      network will be rejected.
                    properties:
                      machine:
                        description: machine contains MTU migration configuration
                          for the machine's uplink. Needs to be migrated along with
                          the default network MTU unless the current uplink MTU already
                          accommodates the default network MTU.
                        properties:
                          from:
                            description: from is the MTU to migrate from.
                            format: int32
                            minimum: 0
                            type: integer
                          to:
                            description: to is the MTU to migrate to.
                            format: int32
                            minimum: 0
                            type: integer
                        type: object
                      network:
                        description: network contains information about MTU migration
                          for the default network. Migrations are only allowed to
                          MTU values lower than the machine's uplink MTU by the minimum
                          appropriate offset.
                        properties:
                          from:
                            description: from is the MTU to migrate from.
                            format: int32
                            minimum: 0
                            type: integer
                          to:
                            description: to is the MTU to migrate to.
                            format: int32
                            minimum: 0
                            type: integer
                        type: object
                    type: object
                  networkType:
                    description: networkType is the target type of network migration.
                      Set this to the target network type to allow changing the default
                      network. If unset, the operation of changing cluster default
                      network plugin will be rejected. The supported values are OpenShiftSDN,
                      OVNKubernetes
                    type: string
                type: object
              observedConfig:
                description: observedConfig holds a sparse config that controller
                  has observed from the cluster state.  It exists in spec because
                  it is an input to the level for the operator
                nullable: true
                type: object
                x-kubernetes-preserve-unknown-fields: true
              operatorLogLevel:
                default: Normal
                description: "operatorLogLevel is an intent based logging for the
                  operator itself.  It does not give fine grained control, but it
                  is a simple way to manage coarse grained logging choices that operators
                  have to interpret for themselves. \n Valid values are: \"Normal\",
                  \"Debug\", \"Trace\", \"TraceAll\". Defaults to \"Normal\"."
                enum:
                - ""
                - Normal
                - Debug
                - Trace
                - TraceAll
                type: string
              serviceNetwork:
                description: serviceNetwork is the ip address pool to use for Service
                  IPs Currently, all existing network providers only support a single
                  value here, but this is an array to allow for growth.
                items:
                  type: string
                type: array
              unsupportedConfigOverrides:
                description: 'unsupportedConfigOverrides holds a sparse config that
                  will override any previously set options.  It only needs to be the
                  fields to override it will end up overlaying in the following order:
                  1. hardcoded defaults 2. observedConfig 3. unsupportedConfigOverrides'
                nullable: true
                type: object
                x-kubernetes-preserve-unknown-fields: true
              useMultiNetworkPolicy:
                description: useMultiNetworkPolicy enables a controller which allows
                  for MultiNetworkPolicy objects to be used on additional networks
                  as created by Multus CNI. MultiNetworkPolicy are similar to NetworkPolicy
                  objects, but NetworkPolicy objects only apply to the primary interface.
                  With MultiNetworkPolicy, you can control the traffic that a pod
                  can receive over the secondary interfaces. If unset, this property
                  defaults to 'false' and MultiNetworkPolicy objects are ignored.
                  If 'disableMultiNetwork' is 'true' then the value of this field
                  is ignored.
                type: boolean
            type: object
          status:
            description: NetworkStatus is detailed operator status, which is distilled
              up to the Network clusteroperator object.
            properties:
              conditions:
                description: conditions is a list of conditions and their status
                items:
                  description: OperatorCondition is just the standard condition fields.
                  properties:
                    lastTransitionTime:
                      format: date-time
                      type: string
                    message:
                      type: string
                    reason:
                      type: string
                    status:
                      type: string
                    type:
                      type: string
                  type: object
                type: array
              generations:
                description: generations are used to determine when an item needs
                  to be reconciled or has changed in a way that needs a reaction.
                items:
                  description: GenerationStatus keeps track of the generation for
                    a given resource so that decisions about forced updates can be
                    made.
                  properties:
                    group:
                      description: group is the group of the thing you're tracking
                      type: string
                    hash:
                      description: hash is an optional field set for resources without
                        generation that are content sensitive like secrets and configmaps
                      type: string
                    lastGeneration:
                      description: lastGeneration is the last generation of the workload
                        controller involved
                      format: int64
                      type: integer
                    name:
                      description: name is the name of the thing you're tracking
                      type: string
                    namespace:
                      description: namespace is where the thing you're tracking is
                      type: string
                    resource:
                      description: resource is the resource type of the thing you're
                        tracking
                      type: string
                  type: object
                type: array
              observedGeneration:
                description: observedGeneration is the last generation change you've
                  dealt with
                format: int64
                type: integer
              readyReplicas:
                description: readyReplicas indicates how many replicas are ready and
                  at the desired state
                format: int32
                type: integer
              version:
                description: version is the level this availability applies to
                type: string
            type: object
        type: object
    served: true
    storage: true
