// Code generated by applyconfiguration-gen. DO NOT EDIT.

package v1

// EgressIPConfigApplyConfiguration represents an declarative configuration of the EgressIPConfig type for use
// with apply.
type EgressIPConfigApplyConfiguration struct {
	ReachabilityTotalTimeoutSeconds *uint32 `json:"reachabilityTotalTimeoutSeconds,omitempty"`
}

// EgressIPConfigApplyConfiguration constructs an declarative configuration of the EgressIPConfig type for use with
// apply.
func EgressIPConfig() *EgressIPConfigApplyConfiguration {
	return &EgressIPConfigApplyConfiguration{}
}

// WithReachabilityTotalTimeoutSeconds sets the ReachabilityTotalTimeoutSeconds field in the declarative configuration to the given value
// and returns the receiver, so that objects can be built by chaining "With" function invocations.
// If called multiple times, the ReachabilityTotalTimeoutSeconds field is set to the value of the last call.
func (b *EgressIPConfigApplyConfiguration) WithReachabilityTotalTimeoutSeconds(value uint32) *EgressIPConfigApplyConfiguration {
	b.ReachabilityTotalTimeoutSeconds = &value
	return b
}
