{
  "schema_version": "1.4.0",
  "id": "GHSA-29r3-8mg2-rxqp",
  "modified": "2022-07-16T00:00:28Z",
  "published": "2022-07-05T00:00:58Z",
  "aliases": [
    "CVE-2022-33971"
  ],
  "details": "Authentication bypass by capture-replay vulnerability exists in Machine automation controller NX7 series all models V1.28 and earlier, Machine automation controller NX1 series all models V1.48 and earlier, and Machine automation controller NJ series all models V 1.48 and earlier, which may allow an adjacent attacker who can analyze the communication between the controller and the specific software used by OMRON internally to cause a denial-of-service (DoS) condition or execute a malicious program.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:A/AC:H/PR:N/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2022-33971"
    },
    {
      "type": "WEB",
      "url": "https://jvn.jp/en/vu/JVNVU97050784/index.html"
    },
    {
      "type": "WEB",
      "url": "https://www.ia.omron.com/product/vulnerability/OMSR-2022-002_en.pdf"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-294"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2022-07-04T02:15:00Z"
  }
}