{
  "schema_version": "1.4.0",
  "id": "GHSA-2qxx-wjxw-fg87",
  "modified": "2024-05-14T18:30:58Z",
  "published": "2024-05-14T18:30:58Z",
  "aliases": [
    "CVE-2024-1913"
  ],
  "details": "\nAn attacker who successfully exploited these vulnerabilities could cause the robot to stop, make the robot controller inaccessible, or execute arbitrary code. \n\nThe vulnerability could potentially be exploited to perform unauthorized actions by an attacker. This vulnerability arises under specific condition when specially crafted message is processed by the system.\n\nBelow are reported vulnerabilities in the Robot Ware versions.\n\n  *  IRC5- RobotWare 6 < 6.15.06 except 6.10.10, and 6.13.07 \n  *  OmniCore- RobotWare 7 < 7.14\n\n",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:N/AC:L/PR:L/UI:N/S:U/C:L/I:L/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2024-1913"
    },
    {
      "type": "WEB",
      "url": "https://search.abb.com/library/Download.aspx?DocumentID=SI20330&LanguageCode=en&DocumentPartId=&Action=Launch"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-787"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2024-05-14T16:16:01Z"
  }
}