# Function _mm512_cvt_roundph_epu16

Source

    pub fn _mm512_cvt_roundph_epu16(a: __m512h, const SAE: i32) -> __m512i

🔬This is a nightly-only experimental API. (`stdarch_x86_avx512_f16` #127213)
Available on (x86 or x86-64) and target feature `avx512fp16` and x86-64 only.
Expand description

Convert packed half-precision (16-bit) floating-point elements in a to packed unsigned 16-bit integers, and store the results in dst.

Exceptions can be suppressed by passing `_MM_FROUND_NO_EXC` in the sae parameter.

Intel’s documentation