# Function _mm256_mask_mov_epi16

1.89.0 · Source

    pub fn _mm256_mask_mov_epi16(src: __m256i, k: __mmask16, a: __m256i) -> __m256i

Available on (x86 or x86-64) and target feature `avx512bw` and target feature `avx512vl` and x86 only.
Expand description

Move packed 16-bit integers from a into dst using writemask k (elements are copied from src when the corresponding mask bit is not set).

Intel’s documentation