# Function _mm_shldv_epi16

1.89.0 · Source

    pub fn _mm_shldv_epi16(a: __m128i, b: __m128i, c: __m128i) -> __m128i

Available on (x86 or x86-64) and target feature `avx512vbmi2` and target feature `avx512vl` and x86-64 only.
Expand description

Concatenate packed 16-bit integers in a and b producing an intermediate 32-bit result. Shift the result left by the amount specified in the corresponding element of c, and store the upper 16-bits in dst.

Intel’s documentation