# Function _mm_mask_storeu_epi16

1.89.0 · Source

    pub unsafe fn _mm_mask_storeu_epi16(
        mem_addr: *mut i16,
        mask: __mmask8,
        a: __m128i,
    )

Available on (x86 or x86-64) and target feature `avx512bw` and target feature `avx512vl` and x86 only.
Expand description

Store packed 16-bit integers from a into memory using writemask k. mem_addr does not need to be aligned on any particular boundary.

Intel’s documentation