# Function _mm512_maskz_maddubs_epi16

1.89.0 · Source

    pub fn _mm512_maskz_maddubs_epi16(
        k: __mmask32,
        a: __m512i,
        b: __m512i,
    ) -> __m512i

Available on (x86 or x86-64) and target feature `avx512bw` and x86-64 only.
Expand description

Multiply packed unsigned 8-bit integers in a by packed signed 8-bit integers in b, producing intermediate signed 16-bit integers. Horizontally add adjacent pairs of intermediate signed 16-bit integers, and pack the saturated results in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation