# Function _mm256_setr_epi16

1.27.0 · Source

    pub fn _mm256_setr_epi16(
        e00: i16,
        e01: i16,
        e02: i16,
        e03: i16,
        e04: i16,
        e05: i16,
        e06: i16,
        e07: i16,
        e08: i16,
        e09: i16,
        e10: i16,
        e11: i16,
        e12: i16,
        e13: i16,
        e14: i16,
        e15: i16,
    ) -> __m256i

Available on (x86 or x86-64) and target feature `avx` and x86-64 only.
Expand description

Sets packed 16-bit integers in returned vector with the supplied values in reverse order.

Intel’s documentation