# SPDX-License-Identifier: GPL-2.0-only OR BSD-2-Clause
%YAML 1.2
---
$id: http://devicetree.org/schemas/timer/brcm,bcmbca-timer.yaml#
$schema: http://devicetree.org/meta-schemas/core.yaml#

title: Broadcom Broadband SoC timer

maintainers:
  - Rafał Miłecki <rafal@milecki.pl>

properties:
  compatible:
    oneOf:
      - const: brcm,bcm6345-timer
        description: >
          An old block with 3 timers.

          It can be found in BCM6345, BCM6838 and BCM63268.
      - const: brcm,bcm63138-timer
        description: >
          Updated block with 4 timers and control regs at the beginning.

          It can be found in newer SoCs, e.g. BCM63138, BCM63148, BCM63381,
          BCM68360, BCM6848, BCM6858, BCM4908.

  reg:
    maxItems: 1

additionalProperties: false

required:
  - reg

examples:
  - |
    timer@fffe0200 {
      compatible = "brcm,bcm6345-timer";
      reg = <0xfffe0200 0x1c>;
    };
