# SPDX-License-Identifier: (GPL-2.0-only OR BSD-2-Clause)
%YAML 1.2
---
$id: http://devicetree.org/schemas/cnxt,cx92755-timer.yaml#
$schema: http://devicetree.org/meta-schemas/core.yaml#

title: Conexant Digicolor SoCs Timer Controller

maintainers:
  - Baruch Siach <baruch@tkos.co.il>

properties:
  compatible:
    const: cnxt,cx92755-timer

  reg:
    maxItems: 1

  interrupts:
    description: Contains 8 interrupts, one for each timer
    items:
      - description: interrupt for timer 0
      - description: interrupt for timer 1
      - description: interrupt for timer 2
      - description: interrupt for timer 3
      - description: interrupt for timer 4
      - description: interrupt for timer 5
      - description: interrupt for timer 6
      - description: interrupt for timer 7

  clocks:
    maxItems: 1

required:
  - compatible
  - reg
  - interrupts
  - clocks

additionalProperties: false

examples:
  - |
    timer@f0000fc0 {
      compatible = "cnxt,cx92755-timer";
      reg = <0xf0000fc0 0x40>;
      interrupts = <19>, <31>, <34>, <35>, <52>, <53>, <54>, <55>;
      clocks = <&main_clk>;
    };
