| # UMAX PowerLook scanners

Index Frontend options: Standard options Advanced options Supported scanners: Power Look series Mirage series Astra series Vista series UC series others Not listed scanners UMAX scanner clones UMAX parallel port scanners Configuration Speed of UMAX scanners SANE-umax homepage SANE homepage XSane homepage |
UMAX scanners
Power Look series:
Name | SCSI-ID | Versions | UTA | ADF | B/W | Gray | Color | Bits/pixel | Optical resolution
PowerLook | PS-2400X | ? | X |  | ok | ok | ok | 1,8,10,24,30 | 600 x 1200
PowerLook II | PL-II | ? | UTA-II |  | ok | ok | ok | 1,8,12,24,36 | 600 x 1200
Power Look III | PowerLook III | all (1.7) | UTA-III |  | ok | ok | ok | 1,8,12,14,24,36,42 | 1200 x 2400
PowerLook 270 | Color Filmscanner____1 | ? | incl |  | bad | bad | bad | 1,8,14,24,42 | 2700 x 2700
PowerLook 270plus | unknown | ? | incl |  | bad | bad | bad | 1,8,14,24,42 | 2700 x 2700
PowerLook 1100 | unknown | ? * | incl |  | ? | ? | ? | 1,8,14,24,42 | 1200 x 2400
PowerLook 2000 | PowerLook 2000 | ? | UTA-2000 |  | ? | ? | ? | 1,8,12,24,36 | 1000 x 2000
PowerLook 2100XL | unknown | ? | UTA-2100XL |  | ? | ? | ? | 1,8,14,24,42 | 800 x 1600
PowerLook 3000 | PowerLook 3000 | all (2.0) | incl |  | ok | ok | ok | 1,8,14,24,42 | 1220 x 3048 3048 x 3048
* Powerlook 1100 is a firewire scanner: not tested UTA = Umax Transparency Adapter, ADF = Automatic Document Feeder (X = supported by scanner, incl = is included) This page has been changed on 16th. decemnber 2001

> Author: Oliver Rauch