# Function _mm_getexp_ps

1.89.0 · Source

    pub fn _mm_getexp_ps(a: __m128) -> __m128

Available on (x86 or x86-64) and target feature `avx512f` and target feature `avx512vl` and x86 only.
Expand description

Convert the exponent of each packed single-precision (32-bit) floating-point element in a to a single-precision (32-bit) floating-point number representing the integer exponent, and store the results in dst. This intrinsic essentially calculates floor(log2(x)) for each element.

Intel’s documentation