# Function _mm256_loadu_ps

1.27.0 · Source

    pub unsafe fn _mm256_loadu_ps(mem_addr: *const f32) -> __m256

Available on (x86 or x86-64) and target feature `avx` and x86 only.
Expand description

Loads 256-bits (composed of 8 packed single-precision (32-bit) floating-point elements) from memory into result. `mem_addr` does not need to be aligned on any particular boundary.

Intel’s documentation