# Function _mm512_loadu_ps

1.89.0 · Source

    pub unsafe fn _mm512_loadu_ps(mem_addr: *const f32) -> __m512

Available on (x86 or x86-64) and target feature `avx512f` and x86 only.
Expand description

Loads 512-bits (composed of 16 packed single-precision (32-bit) floating-point elements) from memory into result. `mem_addr` does not need to be aligned on any particular boundary.

Intel’s documentation