# Function _mm256_mask_div_ps

1.89.0 · Source

    pub fn _mm256_mask_div_ps(
        src: __m256,
        k: __mmask8,
        a: __m256,
        b: __m256,
    ) -> __m256

Available on (x86 or x86-64) and target feature `avx512f` and target feature `avx512vl` and x86 only.
Expand description

Divide packed single-precision (32-bit) floating-point elements in a by packed elements in b, and store the results in dst using writemask k (elements are copied from src when the corresponding mask bit is not set).

Intel’s documentation