# Function _mm_maskz_loadu_ps

1.89.0 · Source

    pub unsafe fn _mm_maskz_loadu_ps(k: __mmask8, mem_addr: *const f32) -> __m128

Available on (x86 or x86-64) and target feature `avx512f` and target feature `avx512vl` and x86-64 only.
Expand description

Load packed single-precision (32-bit) floating-point elements from memory into dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set). mem_addr does not need to be aligned on any particular boundary.

Intel’s documentation