# Function _mm256_mask_compress_ps

1.89.0 · Source

    pub fn _mm256_mask_compress_ps(src: __m256, k: __mmask8, a: __m256) -> __m256

Available on (x86 or x86-64) and target feature `avx512f` and target feature `avx512vl` and x86-64 only.
Expand description

Contiguously store the active single-precision (32-bit) floating-point elements in a (those with their respective bit set in writemask k) to dst, and pass through the remaining elements from src.

Intel’s documentation