# Function _mm_min_ph

Source

    pub fn _mm_min_ph(a: __m128h, b: __m128h) -> __m128h

🔬This is a nightly-only experimental API. (`stdarch_x86_avx512_f16` #127213)
Available on (x86 or x86-64) and target feature `avx512fp16` and target feature `avx512vl` and x86-64 only.
Expand description

Compare packed half-precision (16-bit) floating-point elements in a and b, and store packed minimum values in dst. Does not follow the IEEE Standard for Floating-Point Arithmetic (IEEE 754) minimum value when inputs are NaN or signed-zero values.

Intel’s documentation