# Function _mm_setr_ph

Source

    pub fn _mm_setr_ph(
        e0: f16,
        e1: f16,
        e2: f16,
        e3: f16,
        e4: f16,
        e5: f16,
        e6: f16,
        e7: f16,
    ) -> __m128h

🔬This is a nightly-only experimental API. (`stdarch_x86_avx512_f16` #127213)
Available on (x86 or x86-64) and target feature `avx512fp16` and x86 only.
Expand description

Set packed half-precision (16-bit) floating-point elements in dst with the supplied values in reverse order.

Intel’s documentation