# Function _mm512_maskz_cvtusepi16_epi8

1.89.0 · Source

    pub fn _mm512_maskz_cvtusepi16_epi8(k: __mmask32, a: __m512i) -> __m256i

Available on (x86 or x86-64) and target feature `avx512bw` and x86 only.
Expand description

Convert packed unsigned 16-bit integers in a to packed unsigned 8-bit integers with unsigned saturation, and store the results in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation