# Function _mm256_maskz_expand_epi8

1.89.0 · Source

    pub fn _mm256_maskz_expand_epi8(k: __mmask32, a: __m256i) -> __m256i

Available on (x86 or x86-64) and target feature `avx512vbmi2` and target feature `avx512vl` and x86-64 only.
Expand description

Load contiguous active 8-bit integers from a (those with their respective bit set in mask k), and store the results in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation