# Function _mm256_mask_cvtsepi32_storeu_epi8

1.89.0 · Source

    pub unsafe fn _mm256_mask_cvtsepi32_storeu_epi8(
        mem_addr: *mut i8,
        k: __mmask8,
        a: __m256i,
    )

Available on (x86 or x86-64) and target feature `avx512f` and target feature `avx512vl` and x86-64 only.
Expand description

Convert packed signed 32-bit integers in a to packed 8-bit integers with signed saturation, and store the active results (those with their respective bit set in writemask k) to unaligned memory at base_addr.

Intel’s documentation