# Function _mm_maskz_loadu_epi8

1.89.0 · Source

    pub unsafe fn _mm_maskz_loadu_epi8(k: __mmask16, mem_addr: *const i8) -> __m128i

Available on (x86 or x86-64) and target feature `avx512bw` and target feature `avx512vl` and x86-64 only.
Expand description

Load packed 8-bit integers from memory into dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set). mem_addr does not need to be aligned on any particular boundary.

Intel’s documentation