# Function _mm_mask_loadu_epi8

1.89.0 · Source

    pub unsafe fn _mm_mask_loadu_epi8(
        src: __m128i,
        k: __mmask16,
        mem_addr: *const i8,
    ) -> __m128i

Available on (x86 or x86-64) and target feature `avx512bw` and target feature `avx512vl` and x86-64 only.
Expand description

Load packed 8-bit integers from memory into dst using writemask k (elements are copied from src when the corresponding mask bit is not set). mem_addr does not need to be aligned on any particular boundary.

Intel’s documentation