# Function _ktest_mask16_u8

1.89.0 · Source

    pub unsafe fn _ktest_mask16_u8(
        a: __mmask16,
        b: __mmask16,
        and_not: *mut u8,
    ) -> u8

Available on (x86 or x86-64) and target feature `avx512dq` and x86 only.
Expand description

Compute the bitwise AND of 16-bit masks a and b, and if the result is all zeros, store 1 in dst, otherwise store 0 in dst. Compute the bitwise NOT of a and then AND with b, if the result is all zeros, store 1 in and_not, otherwise store 0 in and_not.

Intel’s Documentation