## Keyboard shortcuts

Press `←` or `→` to navigate between chapters

Press `S` or `/` to search in the book

Press `?` to show this help

Press `Esc` to hide this help

# `small-data-threshold`

This flag controls the maximum static variable size that may be included in the "small data sections" (.sdata, .sbss) supported by some architectures (RISCV, MIPS, M68K, Hexagon). Can be set to `0` to disable the use of small data sections.

Target support is indicated by the `small_data_threshold_support` target option which can be:

- `none` (`SmallDataThresholdSupport::None`) for no support
- `default-for-arch` (`SmallDataThresholdSupport::DefaultForArch`) which is automatically translated into an appropriate value for the target.
- `llvm-module-flag=<flag_name>` (`SmallDataThresholdSupport::LlvmModuleFlag`) for specifying the threshold via an LLVM module flag
- `llvm-arg=<arg_name>` (`SmallDataThresholdSupport::LlvmArg`) for specifying the threshold via an LLVM argument.